PKIX1Explicit88 { iso(1) identified-organization(3) dod(6) internet(1)
  security(5) mechanisms(5) pkix(7) id-mod(0) id-pkix1-explicit(18) }

DEFINITIONS EXPLICIT TAGS ::=

BEGIN

-- EXPORTS ALL --

-- IMPORTS NONE --

-- UNIVERSAL Types defined in 1993 and 1998 ASN.1
-- and required by this specification

-- pycrate: UniversalString, BMPString and UTF8String already in the builtin types

--UniversalString ::= [UNIVERSAL 28] IMPLICIT OCTET STRING
        -- UniversalString is defined in ASN.1:1993

--BMPString ::= [UNIVERSAL 30] IMPLICIT OCTET STRING
      -- BMPString is the subtype of UniversalString and models
      -- the Basic Multilingual Plane of ISO/IEC 10646

--UTF8String ::= [UNIVERSAL 12] IMPLICIT OCTET STRING
      -- The content of this type conforms to RFC 3629.

-- PKIX specific OIDs

id-pkix  OBJECT IDENTIFIER  ::=
         { iso(1) identified-organization(3) dod(6) internet(1)
                    security(5) mechanisms(5) pkix(7) }

-- PKIX arcs

id-pe OBJECT IDENTIFIER ::= { id-pkix 1 }
        -- arc for private certificate extensions
id-qt OBJECT IDENTIFIER ::= { id-pkix 2 }
        -- arc for policy qualifier types
id-kp OBJECT IDENTIFIER ::= { id-pkix 3 }
        -- arc for extended key purpose OIDS
id-ad OBJECT IDENTIFIER ::= { id-pkix 48 }
        -- arc for access descriptors

-- policyQualifierIds for Internet policy qualifiers

id-qt-cps      OBJECT IDENTIFIER ::=  { id-qt 1 }
      -- OID for CPS qualifier
id-qt-unotice  OBJECT IDENTIFIER ::=  { id-qt 2 }
      -- OID for user notice qualifier

-- access descriptor definitions

id-ad-ocsp         OBJECT IDENTIFIER ::= { id-ad 1 }
id-ad-caIssuers    OBJECT IDENTIFIER ::= { id-ad 2 }
id-ad-timeStamping OBJECT IDENTIFIER ::= { id-ad 3 }
id-ad-caRepository OBJECT IDENTIFIER ::= { id-ad 5 }

-- attribute data types

Attribute               ::= SEQUENCE {
      type             AttributeType,
      values    SET OF AttributeValue }
            -- at least one value is required

AttributeType           ::= OBJECT IDENTIFIER

AttributeValue          ::= ANY -- DEFINED BY AttributeType

AttributeTypeAndValue   ::= SEQUENCE {
        type    AttributeType,
        value   AttributeValue }

-- suggested naming attributes: Definition of the following
--   information object set may be augmented to meet local
--   requirements.  Note that deleting members of the set may
--   prevent interoperability with conforming implementations.
-- presented in pairs: the AttributeType followed by the
--   type definition for the corresponding AttributeValue

-- Arc for standard naming attributes

id-at OBJECT IDENTIFIER ::= { joint-iso-ccitt(2) ds(5) 4 }

-- Naming attributes of type X520name

id-at-name                AttributeType ::= { id-at 41 }
id-at-surname             AttributeType ::= { id-at  4 }
id-at-givenName           AttributeType ::= { id-at 42 }
id-at-initials            AttributeType ::= { id-at 43 }
id-at-generationQualifier AttributeType ::= { id-at 44 }

-- Naming attributes of type X520Name:
--   X520name ::= DirectoryString (SIZE (1..ub-name))
--
-- Expanded to avoid parameterized type:
X520name ::= CHOICE {
      teletexString     TeletexString   (SIZE (1..ub-name)),
      printableString   PrintableString (SIZE (1..ub-name)),
      universalString   UniversalString (SIZE (1..ub-name)),
      utf8String        UTF8String      (SIZE (1..ub-name)),
      bmpString         BMPString       (SIZE (1..ub-name)) }

-- Naming attributes of type X520CommonName

id-at-commonName        AttributeType ::= { id-at 3 }

-- Naming attributes of type X520CommonName:
--   X520CommonName ::= DirectoryName (SIZE (1..ub-common-name))
--
-- Expanded to avoid parameterized type:
X520CommonName ::= CHOICE {
      teletexString     TeletexString   (SIZE (1..ub-common-name)),
      printableString   PrintableString (SIZE (1..ub-common-name)),
      universalString   UniversalString (SIZE (1..ub-common-name)),
      utf8String        UTF8String      (SIZE (1..ub-common-name)),
      bmpString         BMPString       (SIZE (1..ub-common-name)) }

-- Naming attributes of type X520LocalityName

id-at-localityName      AttributeType ::= { id-at 7 }

-- Naming attributes of type X520LocalityName:
--   X520LocalityName ::= DirectoryName (SIZE (1..ub-locality-name))
--
-- Expanded to avoid parameterized type:
X520LocalityName ::= CHOICE {
      teletexString     TeletexString   (SIZE (1..ub-locality-name)),
      printableString   PrintableString (SIZE (1..ub-locality-name)),
      universalString   UniversalString (SIZE (1..ub-locality-name)),
      utf8String        UTF8String      (SIZE (1..ub-locality-name)),
      bmpString         BMPString       (SIZE (1..ub-locality-name)) }

-- Naming attributes of type X520StateOrProvinceName

id-at-stateOrProvinceName AttributeType ::= { id-at 8 }

-- Naming attributes of type X520StateOrProvinceName:
--   X520StateOrProvinceName ::= DirectoryName (SIZE (1..ub-state-name))
--
-- Expanded to avoid parameterized type:
X520StateOrProvinceName ::= CHOICE {
      teletexString     TeletexString   (SIZE (1..ub-state-name)),
      printableString   PrintableString (SIZE (1..ub-state-name)),
      universalString   UniversalString (SIZE (1..ub-state-name)),
      utf8String        UTF8String      (SIZE (1..ub-state-name)),
      bmpString         BMPString       (SIZE (1..ub-state-name)) }

-- Naming attributes of type X520OrganizationName

id-at-organizationName  AttributeType ::= { id-at 10 }

-- Naming attributes of type X520OrganizationName:
--   X520OrganizationName ::=
--          DirectoryName (SIZE (1..ub-organization-name))
--
-- Expanded to avoid parameterized type:
X520OrganizationName ::= CHOICE {
      teletexString     TeletexString
                          (SIZE (1..ub-organization-name)),
      printableString   PrintableString
                          (SIZE (1..ub-organization-name)),
      universalString   UniversalString
                          (SIZE (1..ub-organization-name)),
      utf8String        UTF8String
                          (SIZE (1..ub-organization-name)),
      bmpString         BMPString
                          (SIZE (1..ub-organization-name))  }

-- Naming attributes of type X520OrganizationalUnitName

id-at-organizationalUnitName AttributeType ::= { id-at 11 }

-- Naming attributes of type X520OrganizationalUnitName:
--   X520OrganizationalUnitName ::=
--          DirectoryName (SIZE (1..ub-organizational-unit-name))
--
-- Expanded to avoid parameterized type:
X520OrganizationalUnitName ::= CHOICE {
      teletexString     TeletexString
                          (SIZE (1..ub-organizational-unit-name)),
      printableString   PrintableString
                          (SIZE (1..ub-organizational-unit-name)),
      universalString   UniversalString
                          (SIZE (1..ub-organizational-unit-name)),
      utf8String        UTF8String
                          (SIZE (1..ub-organizational-unit-name)),
      bmpString         BMPString
                          (SIZE (1..ub-organizational-unit-name)) }

-- Naming attributes of type X520Title

id-at-title             AttributeType ::= { id-at 12 }

-- Naming attributes of type X520Title:
--   X520Title ::= DirectoryName (SIZE (1..ub-title))
--
-- Expanded to avoid parameterized type:
X520Title ::= CHOICE {
      teletexString     TeletexString   (SIZE (1..ub-title)),
      printableString   PrintableString (SIZE (1..ub-title)),
      universalString   UniversalString (SIZE (1..ub-title)),
      utf8String        UTF8String      (SIZE (1..ub-title)),
      bmpString         BMPString       (SIZE (1..ub-title)) }

-- Naming attributes of type X520dnQualifier

id-at-dnQualifier       AttributeType ::= { id-at 46 }

X520dnQualifier ::=     PrintableString

-- Naming attributes of type X520countryName (digraph from IS 3166)

id-at-countryName       AttributeType ::= { id-at 6 }

X520countryName ::=     PrintableString (SIZE (2))

-- Naming attributes of type X520SerialNumber

id-at-serialNumber      AttributeType ::= { id-at 5 }

X520SerialNumber ::=    PrintableString (SIZE (1..ub-serial-number))

-- Naming attributes of type X520Pseudonym

id-at-pseudonym         AttributeType ::= { id-at 65 }

-- Naming attributes of type X520Pseudonym:
--   X520Pseudonym ::= DirectoryName (SIZE (1..ub-pseudonym))
--
-- Expanded to avoid parameterized type:
X520Pseudonym ::= CHOICE {
   teletexString     TeletexString   (SIZE (1..ub-pseudonym)),
   printableString   PrintableString (SIZE (1..ub-pseudonym)),
   universalString   UniversalString (SIZE (1..ub-pseudonym)),
   utf8String        UTF8String      (SIZE (1..ub-pseudonym)),
   bmpString         BMPString       (SIZE (1..ub-pseudonym)) }

-- Naming attributes of type DomainComponent (from RFC 4519)

id-domainComponent   AttributeType ::= { 0 9 2342 19200300 100 1 25 }

DomainComponent ::=  IA5String

-- Legacy attributes

pkcs-9 OBJECT IDENTIFIER ::=
       { iso(1) member-body(2) us(840) rsadsi(113549) pkcs(1) 9 }

id-emailAddress      AttributeType ::= { pkcs-9 1 }

EmailAddress ::=     IA5String (SIZE (1..ub-emailaddress-length))

-- naming data types --

Name ::= CHOICE { -- only one possibility for now --
      rdnSequence  RDNSequence }

RDNSequence ::= SEQUENCE OF RelativeDistinguishedName

DistinguishedName ::=   RDNSequence

RelativeDistinguishedName ::= SET SIZE (1..MAX) OF AttributeTypeAndValue

-- Directory string type --

DirectoryString ::= CHOICE {
      teletexString       TeletexString   (SIZE (1..MAX)),
      printableString     PrintableString (SIZE (1..MAX)),
      universalString     UniversalString (SIZE (1..MAX)),
      utf8String          UTF8String      (SIZE (1..MAX)),
      bmpString           BMPString       (SIZE (1..MAX)) }

-- certificate and CRL specific structures begin here

Certificate  ::=  SEQUENCE  {
     tbsCertificate       TBSCertificate,
     signatureAlgorithm   AlgorithmIdentifier,
     signature            BIT STRING  }

TBSCertificate  ::=  SEQUENCE  {
     version         [0]  Version DEFAULT v1,
     serialNumber         CertificateSerialNumber,
     signature            AlgorithmIdentifier,
     issuer               Name,
     validity             Validity,
     subject              Name,
     subjectPublicKeyInfo SubjectPublicKeyInfo,
     issuerUniqueID  [1]  IMPLICIT UniqueIdentifier OPTIONAL,
                          -- If present, version MUST be v2 or v3
     subjectUniqueID [2]  IMPLICIT UniqueIdentifier OPTIONAL,
                          -- If present, version MUST be v2 or v3
     extensions      [3]  Extensions OPTIONAL
                          -- If present, version MUST be v3 --  }

Version  ::=  INTEGER  {  v1(0), v2(1), v3(2)  }

CertificateSerialNumber  ::=  INTEGER

Validity ::= SEQUENCE {
     notBefore      Time,
     notAfter       Time  }

Time ::= CHOICE {
     utcTime        UTCTime,
     generalTime    GeneralizedTime }

UniqueIdentifier  ::=  BIT STRING

SubjectPublicKeyInfo  ::=  SEQUENCE  {
     algorithm            AlgorithmIdentifier,
     subjectPublicKey     BIT STRING  }

Extensions  ::=  SEQUENCE SIZE (1..MAX) OF Extension

Extension  ::=  SEQUENCE  {
     extnID      OBJECT IDENTIFIER,
     critical    BOOLEAN DEFAULT FALSE,
     extnValue   OCTET STRING
                 -- contains the DER encoding of an ASN.1 value
                 -- corresponding to the extension type identified
                 -- by extnID
     }

-- CRL structures

CertificateList  ::=  SEQUENCE  {
     tbsCertList          TBSCertList,
     signatureAlgorithm   AlgorithmIdentifier,
     signature            BIT STRING  }

TBSCertList  ::=  SEQUENCE  {
     version                 Version OPTIONAL,
                                   -- if present, MUST be v2
     signature               AlgorithmIdentifier,
     issuer                  Name,
     thisUpdate              Time,
     nextUpdate              Time OPTIONAL,
     revokedCertificates     SEQUENCE OF SEQUENCE  {
          userCertificate         CertificateSerialNumber,
          revocationDate          Time,
          crlEntryExtensions      Extensions OPTIONAL
                                   -- if present, version MUST be v2
                               }  OPTIONAL,
     crlExtensions           [0] Extensions OPTIONAL }
                                   -- if present, version MUST be v2

-- Version, Time, CertificateSerialNumber, and Extensions were
-- defined earlier for use in the certificate structure

AlgorithmIdentifier  ::=  SEQUENCE  {
     algorithm               OBJECT IDENTIFIER,
     parameters              ANY DEFINED BY algorithm OPTIONAL  }
                                -- contains a value of the type
                                -- registered for use with the
                                -- algorithm object identifier value

-- X.400 address syntax starts here

ORAddress ::= SEQUENCE {
   built-in-standard-attributes BuiltInStandardAttributes,
   built-in-domain-defined-attributes
                   BuiltInDomainDefinedAttributes OPTIONAL,
   -- see also teletex-domain-defined-attributes
   extension-attributes ExtensionAttributes OPTIONAL }

-- Built-in Standard Attributes

BuiltInStandardAttributes ::= SEQUENCE {
   country-name                  CountryName OPTIONAL,
   administration-domain-name    AdministrationDomainName OPTIONAL,
   network-address           [0] IMPLICIT NetworkAddress OPTIONAL,
     -- see also extended-network-address
   terminal-identifier       [1] IMPLICIT TerminalIdentifier OPTIONAL,
   private-domain-name       [2] PrivateDomainName OPTIONAL,
   organization-name         [3] IMPLICIT OrganizationName OPTIONAL,
     -- see also teletex-organization-name
   numeric-user-identifier   [4] IMPLICIT NumericUserIdentifier
                                 OPTIONAL,
   personal-name             [5] IMPLICIT PersonalName OPTIONAL,
     -- see also teletex-personal-name
   organizational-unit-names [6] IMPLICIT OrganizationalUnitNames
                                 OPTIONAL }
     -- see also teletex-organizational-unit-names

CountryName ::= [APPLICATION 1] CHOICE {
   x121-dcc-code         NumericString
                           (SIZE (ub-country-name-numeric-length)),
   iso-3166-alpha2-code  PrintableString
                           (SIZE (ub-country-name-alpha-length)) }

AdministrationDomainName ::= [APPLICATION 2] CHOICE {
   numeric   NumericString   (SIZE (0..ub-domain-name-length)),
   printable PrintableString (SIZE (0..ub-domain-name-length)) }

NetworkAddress ::= X121Address  -- see also extended-network-address

X121Address ::= NumericString (SIZE (1..ub-x121-address-length))

TerminalIdentifier ::= PrintableString (SIZE (1..ub-terminal-id-length))

PrivateDomainName ::= CHOICE {
   numeric   NumericString   (SIZE (1..ub-domain-name-length)),
   printable PrintableString (SIZE (1..ub-domain-name-length)) }

OrganizationName ::= PrintableString
                            (SIZE (1..ub-organization-name-length))
  -- see also teletex-organization-name

NumericUserIdentifier ::= NumericString
                            (SIZE (1..ub-numeric-user-id-length))

PersonalName ::= SET {
   surname     [0] IMPLICIT PrintableString
                    (SIZE (1..ub-surname-length)),
   given-name  [1] IMPLICIT PrintableString
                    (SIZE (1..ub-given-name-length)) OPTIONAL,
   initials    [2] IMPLICIT PrintableString
                    (SIZE (1..ub-initials-length)) OPTIONAL,
   generation-qualifier [3] IMPLICIT PrintableString
                    (SIZE (1..ub-generation-qualifier-length))
                    OPTIONAL }
  -- see also teletex-personal-name

OrganizationalUnitNames ::= SEQUENCE SIZE (1..ub-organizational-units)
                             OF OrganizationalUnitName
  -- see also teletex-organizational-unit-names

OrganizationalUnitName ::= PrintableString (SIZE
                    (1..ub-organizational-unit-name-length))

-- Built-in Domain-defined Attributes

BuiltInDomainDefinedAttributes ::= SEQUENCE SIZE
                    (1..ub-domain-defined-attributes) OF
                    BuiltInDomainDefinedAttribute

BuiltInDomainDefinedAttribute ::= SEQUENCE {
   type PrintableString (SIZE
                   (1..ub-domain-defined-attribute-type-length)),
   value PrintableString (SIZE
                   (1..ub-domain-defined-attribute-value-length)) }

-- Extension Attributes

ExtensionAttributes ::= SET SIZE (1..ub-extension-attributes) OF
               ExtensionAttribute

ExtensionAttribute ::=  SEQUENCE {
   extension-attribute-type [0] IMPLICIT INTEGER
                   (0..ub-extension-attributes),
   extension-attribute-value [1]
                   ANY DEFINED BY extension-attribute-type }

-- Extension types and attribute values

common-name INTEGER ::= 1

CommonName ::= PrintableString (SIZE (1..ub-common-name-length))

teletex-common-name INTEGER ::= 2

TeletexCommonName ::= TeletexString (SIZE (1..ub-common-name-length))

teletex-organization-name INTEGER ::= 3

TeletexOrganizationName ::=
                TeletexString (SIZE (1..ub-organization-name-length))

teletex-personal-name INTEGER ::= 4

TeletexPersonalName ::= SET {
   surname     [0] IMPLICIT TeletexString
                    (SIZE (1..ub-surname-length)),
   given-name  [1] IMPLICIT TeletexString
                    (SIZE (1..ub-given-name-length)) OPTIONAL,
   initials    [2] IMPLICIT TeletexString
                    (SIZE (1..ub-initials-length)) OPTIONAL,
   generation-qualifier [3] IMPLICIT TeletexString
                    (SIZE (1..ub-generation-qualifier-length))
                    OPTIONAL }

teletex-organizational-unit-names INTEGER ::= 5

TeletexOrganizationalUnitNames ::= SEQUENCE SIZE
      (1..ub-organizational-units) OF TeletexOrganizationalUnitName

TeletexOrganizationalUnitName ::= TeletexString
                  (SIZE (1..ub-organizational-unit-name-length))

pds-name INTEGER ::= 7

PDSName ::= PrintableString (SIZE (1..ub-pds-name-length))

physical-delivery-country-name INTEGER ::= 8

PhysicalDeliveryCountryName ::= CHOICE {
   x121-dcc-code NumericString (SIZE (ub-country-name-numeric-length)),
   iso-3166-alpha2-code PrintableString
                               (SIZE (ub-country-name-alpha-length)) }

postal-code INTEGER ::= 9

PostalCode ::= CHOICE {
   numeric-code   NumericString (SIZE (1..ub-postal-code-length)),
   printable-code PrintableString (SIZE (1..ub-postal-code-length)) }

physical-delivery-office-name INTEGER ::= 10

PhysicalDeliveryOfficeName ::= PDSParameter

physical-delivery-office-number INTEGER ::= 11

PhysicalDeliveryOfficeNumber ::= PDSParameter

extension-OR-address-components INTEGER ::= 12

ExtensionORAddressComponents ::= PDSParameter

physical-delivery-personal-name INTEGER ::= 13

PhysicalDeliveryPersonalName ::= PDSParameter

physical-delivery-organization-name INTEGER ::= 14

PhysicalDeliveryOrganizationName ::= PDSParameter

extension-physical-delivery-address-components INTEGER ::= 15

ExtensionPhysicalDeliveryAddressComponents ::= PDSParameter

unformatted-postal-address INTEGER ::= 16

UnformattedPostalAddress ::= SET {
   printable-address SEQUENCE SIZE (1..ub-pds-physical-address-lines)
        OF PrintableString (SIZE (1..ub-pds-parameter-length)) OPTIONAL,
   teletex-string TeletexString
        (SIZE (1..ub-unformatted-address-length)) OPTIONAL }

street-address INTEGER ::= 17

StreetAddress ::= PDSParameter

post-office-box-address INTEGER ::= 18

PostOfficeBoxAddress ::= PDSParameter

poste-restante-address INTEGER ::= 19

PosteRestanteAddress ::= PDSParameter

unique-postal-name INTEGER ::= 20

UniquePostalName ::= PDSParameter

local-postal-attributes INTEGER ::= 21

LocalPostalAttributes ::= PDSParameter

PDSParameter ::= SET {
   printable-string PrintableString
                (SIZE(1..ub-pds-parameter-length)) OPTIONAL,
   teletex-string TeletexString
                (SIZE(1..ub-pds-parameter-length)) OPTIONAL }

extended-network-address INTEGER ::= 22

ExtendedNetworkAddress ::= CHOICE {
   e163-4-address SEQUENCE {
      number      [0] IMPLICIT NumericString
                       (SIZE (1..ub-e163-4-number-length)),
      sub-address [1] IMPLICIT NumericString
                       (SIZE (1..ub-e163-4-sub-address-length))
                       OPTIONAL },
   psap-address   [0] IMPLICIT PresentationAddress }

PresentationAddress ::= SEQUENCE {
    pSelector     [0] EXPLICIT OCTET STRING OPTIONAL,
    sSelector     [1] EXPLICIT OCTET STRING OPTIONAL,
    tSelector     [2] EXPLICIT OCTET STRING OPTIONAL,
    nAddresses    [3] EXPLICIT SET SIZE (1..MAX) OF OCTET STRING }

terminal-type  INTEGER ::= 23

TerminalType ::= INTEGER {
   telex        (3),
   teletex      (4),
   g3-facsimile (5),
   g4-facsimile (6),
   ia5-terminal (7),
   videotex     (8) } (0..ub-integer-options)

-- Extension Domain-defined Attributes

teletex-domain-defined-attributes INTEGER ::= 6

TeletexDomainDefinedAttributes ::= SEQUENCE SIZE
   (1..ub-domain-defined-attributes) OF TeletexDomainDefinedAttribute

TeletexDomainDefinedAttribute ::= SEQUENCE {
        type TeletexString
               (SIZE (1..ub-domain-defined-attribute-type-length)),
        value TeletexString
               (SIZE (1..ub-domain-defined-attribute-value-length)) }

--  specifications of Upper Bounds MUST be regarded as mandatory
--  from Annex B of ITU-T X.411 Reference Definition of MTS Parameter
--  Upper Bounds

-- Upper Bounds
ub-name INTEGER ::= 32768
ub-common-name INTEGER ::= 64
ub-locality-name INTEGER ::= 128
ub-state-name INTEGER ::= 128
ub-organization-name INTEGER ::= 64
ub-organizational-unit-name INTEGER ::= 64
ub-title INTEGER ::= 64
ub-serial-number INTEGER ::= 64
ub-match INTEGER ::= 128
ub-emailaddress-length INTEGER ::= 255
ub-common-name-length INTEGER ::= 64
ub-country-name-alpha-length INTEGER ::= 2
ub-country-name-numeric-length INTEGER ::= 3
ub-domain-defined-attributes INTEGER ::= 4
ub-domain-defined-attribute-type-length INTEGER ::= 8
ub-domain-defined-attribute-value-length INTEGER ::= 128
ub-domain-name-length INTEGER ::= 16
ub-extension-attributes INTEGER ::= 256
ub-e163-4-number-length INTEGER ::= 15
ub-e163-4-sub-address-length INTEGER ::= 40
ub-generation-qualifier-length INTEGER ::= 3
ub-given-name-length INTEGER ::= 16
ub-initials-length INTEGER ::= 5
ub-integer-options INTEGER ::= 256
ub-numeric-user-id-length INTEGER ::= 32
ub-organization-name-length INTEGER ::= 64
ub-organizational-unit-name-length INTEGER ::= 32
ub-organizational-units INTEGER ::= 4
ub-pds-name-length INTEGER ::= 16
ub-pds-parameter-length INTEGER ::= 30
ub-pds-physical-address-lines INTEGER ::= 6
ub-postal-code-length INTEGER ::= 16
ub-pseudonym INTEGER ::= 128
ub-surname-length INTEGER ::= 40
ub-terminal-id-length INTEGER ::= 24
ub-unformatted-address-length INTEGER ::= 180
ub-x121-address-length INTEGER ::= 16

-- Note - upper bounds on string types, such as TeletexString, are
-- measured in characters.  Excepting PrintableString or IA5String, a
-- significantly greater number of octets will be required to hold
-- such a value.  As a minimum, 16 octets, or twice the specified
-- upper bound, whichever is the larger, should be allowed for
-- TeletexString.  For UTF8String or UniversalString at least four
-- times the upper bound should be allowed.

END

