Cmp-Mod V01 Genere par PcbNew le Di 21 Jun 2011 15:43:44 CEST

BeginCmp
TimeStamp = 4DCD07C6
Path = /4DC51F05
Reference = P3;
ValeurCmp = REBEL;
IdModule  = FFC_REBELSIM;
EndCmp

BeginCmp
TimeStamp = 4DCD07C7
Path = /4DCBE233
Reference = J2;
ValeurCmp = SERIAL;
IdModule  = JACK_2.5;
EndCmp

BeginCmp
TimeStamp = 4DCD07C8
Path = /4CF5471F
Reference = D5;
ValeurCmp = GREEN;
IdModule  = LED-0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07CA
Path = /4CF54717
Reference = D4;
ValeurCmp = RED;
IdModule  = LED-0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07CB
Path = /4CFCD6C9
Reference = P1;
ValeurCmp = JTAG;
IdModule  = pin_array_10x2;
EndCmp

BeginCmp
TimeStamp = 4DCD07CC
Path = /4DC683ED
Reference = JP2;
ValeurCmp = ERASE;
IdModule  = PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = 4DCD07CE
Path = /4DC68259
Reference = JP1;
ValeurCmp = TEST;
IdModule  = PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = 4DD21AFA
Path = /4DC804A6
Reference = BT1;
ValeurCmp = 4.5-6V;
IdModule  = PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = 4DCD07D5
Path = /4CE915DE
Reference = X1;
ValeurCmp = 18.432MHz;
IdModule  = Q_49U3HMS;
EndCmp

BeginCmp
TimeStamp = 4DCD07D7
Path = /4DC5A30D
Reference = R18;
ValeurCmp = 10k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07D9
Path = /4DC799F2
Reference = R17;
ValeurCmp = 10k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07DB
Path = /4DC7A441
Reference = R16;
ValeurCmp = 10K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07DF
Path = /4DC555D0
Reference = R14;
ValeurCmp = 150R;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07E1
Path = /4CF7BAEE
Reference = R13;
ValeurCmp = 150R;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07E3
Path = /4D0206C7
Reference = R12;
ValeurCmp = 100k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07E5
Path = /4D020DC6
Reference = R11;
ValeurCmp = 1k5;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07E7
Path = /4DC79EA7
Reference = R10;
ValeurCmp = 27R;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07E9
Path = /4DC79EAD
Reference = R9;
ValeurCmp = 27R;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07EB
Path = /4CE9A6AE
Reference = R8;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07ED
Path = /4CE9A6A9
Reference = R7;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07EF
Path = /4CE9A6A5
Reference = R6;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07F1
Path = /4CE9A69A
Reference = R5;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07F3
Path = /4CE9A68C
Reference = R4;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07F5
Path = /4DC79ECE
Reference = R3;
ValeurCmp = 1K5;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07F7
Path = /4DC79E9A
Reference = R2;
ValeurCmp = 10K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07F9
Path = /4DC79ED1
Reference = R1;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07FB
Path = /4DC68E45
Reference = C23;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07FD
Path = /4DC6A5D9
Reference = C22;
ValeurCmp = 1uF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD07FF
Path = /4DC6A5CB
Reference = C21;
ValeurCmp = 1uF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD0801
Path = /4D020EDF
Reference = C20;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD0803
Path = /4DC664E0
Reference = C19;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD0805
Path = /4CE91633
Reference = C18;
ValeurCmp = 10pF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD0807
Path = /4CE9162F
Reference = C17;
ValeurCmp = 10pF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD0809
Path = /4DC664DD
Reference = C16;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD080B
Path = /4D020ED8
Reference = C15;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD080D
Path = /4DC6A5DE
Reference = C14;
ValeurCmp = 1uF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD080F
Path = /4DC79EDC
Reference = C13;
ValeurCmp = 15pF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD0811
Path = /4DC8F97A
Reference = C12;
ValeurCmp = 2.2uF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD0813
Path = /4DC79ED8
Reference = C11;
ValeurCmp = 15pF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD0815
Path = /4D020DCD
Reference = C10;
ValeurCmp = 1nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD0817
Path = /4D020BEB
Reference = C9;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD0819
Path = /4D020BDE
Reference = C7;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD081B
Path = /4D020DD3
Reference = C6;
ValeurCmp = 10nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DFF297E
Path = /4DC79EDF
Reference = C5;
ValeurCmp = 33pF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD081F
Path = /4DC66392
Reference = C4;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD0821
Path = /4D037E30
Reference = C3;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD0823
Path = /4DC8F975
Reference = C1;
ValeurCmp = 2.2uF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DCD0824
Path = /4DC68E1D
Reference = FB2;
ValeurCmp = FILTER;
IdModule  = SM0805;
EndCmp

BeginCmp
TimeStamp = 4DCD0826
Path = /4DC79E48
Reference = FB1;
ValeurCmp = FILTER;
IdModule  = SM0805;
EndCmp

BeginCmp
TimeStamp = 4DCD0828
Path = /4DCB8C0D
Reference = D3;
ValeurCmp = 1N5819;
IdModule  = SOD123;
EndCmp

BeginCmp
TimeStamp = 4DCD082A
Path = /4DCB8C13
Reference = D2;
ValeurCmp = 1N5819;
IdModule  = SOD123;
EndCmp

BeginCmp
TimeStamp = 4DCD082C
Path = /4DC7A27C
Reference = D1;
ValeurCmp = Schottky;
IdModule  = SOD123;
EndCmp

BeginCmp
TimeStamp = 4DCD082D
Path = /4DC5A250
Reference = U1;
ValeurCmp = FLASH;
IdModule  = SOIC8;
EndCmp

BeginCmp
TimeStamp = 4DCD0831
Path = /4CE84486
Reference = IC3;
ValeurCmp = AT91SAM7S;
IdModule  = TQFP_64;
EndCmp

BeginCmp
TimeStamp = 4DCD07D1
Path = /4CE9ADCF
Reference = P2;
ValeurCmp = DEBUG;
IdModule  = PIN_ARRAY-6X1;
EndCmp

BeginCmp
TimeStamp = 4DFFCD2F
Path = /4DC7A43A
Reference = Q2;
ValeurCmp = BC847;
IdModule  = SOT23_BC847;
EndCmp

BeginCmp
TimeStamp = 4DCD0827
Path = /4DC7A1CA
Reference = Q1;
ValeurCmp = BC847;
IdModule  = SOT23_BC847;
EndCmp

BeginCmp
TimeStamp = 4DCD07D4
Path = /4D020733
Reference = SW1;
ValeurCmp = RESET;
IdModule  = PUSH_BUTTON;
EndCmp

BeginCmp
TimeStamp = 4DCD07D2
Path = /4DC6852C
Reference = SW2;
ValeurCmp = BOOTLOADER;
IdModule  = PUSH_BUTTON;
EndCmp

BeginCmp
TimeStamp = 4DD21AF7
Path = /4CFAC6EA
Reference = J1;
ValeurCmp = USB;
IdModule  = USB-MINI-B_UX60;
EndCmp

BeginCmp
TimeStamp = 4DCD07D6
Path = /4DC8FA06
Reference = P4;
ValeurCmp = SIM;
IdModule  = SIM_AMPHENOL;
EndCmp

BeginCmp
TimeStamp = 4DCD0830
Path = /4DC6A187
Reference = IC4;
ValeurCmp = CB3Q3244;
IdModule  = SSOP20_BDQ;
EndCmp

BeginCmp
TimeStamp = 4DFFA0F3
Path = /4DFF9902
Reference = R22;
ValeurCmp = 100k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DFFA2A6
Path = /4DFF746C
Reference = R21;
ValeurCmp = 10k1%;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DFFA0F7
Path = /4DFF7469
Reference = R20;
ValeurCmp = 10k1%;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DFFA0F9
Path = /4DFF73B0
Reference = R19;
ValeurCmp = 100K;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DFFA0FB
Path = /4DFF9964
Reference = C24;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = 4DFFA0FC
Path = /4DFF9774
Reference = IC5;
ValeurCmp = FPF2005;
IdModule  = SOT353;
EndCmp

BeginCmp
TimeStamp = 4DCD082E
Path = /4DFF8B97
Reference = IC2;
ValeurCmp = LDO;
IdModule  = SOT26;
EndCmp

EndListe
