<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="50.32" x2="0" y2="3.18" width="0" layer="20"/>
<wire x1="0" y1="3.18" x2="3.18" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.18" y1="0" x2="99" y2="0" width="0" layer="20"/>
<wire x1="99" y1="0" x2="100" y2="1" width="0" layer="20" curve="90"/>
<wire x1="100" y1="1" x2="100" y2="52.5" width="0" layer="20"/>
<wire x1="100" y1="52.5" x2="99" y2="53.5" width="0" layer="20" curve="90"/>
<wire x1="99" y1="53.5" x2="3.18" y2="53.5" width="0" layer="20"/>
<wire x1="3.18" y1="53.5" x2="0" y2="50.32" width="0" layer="20" curve="90"/>
<text>smart card FPC adapter
(C) 2020 sysmocom - s.f.m.c. GmbH</text>
<text>smart card FPC adapter
(C) 2020 sysmocom - s.f.m.c. GmbH</text>
<text>smart card FPC adapter
(C) 2020 sysmocom - s.f.m.c. GmbH</text>
<text>smart card FPC adapter
(C) 2020 sysmocom - s.f.m.c. GmbH</text>
</plain>
<libraries>
<library name="iso7816-card">
<packages>
<package name="ISO7816_CARD">
<description>Smart Card as per ISO7816-2</description>
</package>
</packages>
</library>
<library name="laforge">
<description>&lt;b&gt;PCB Matrix Packages&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="FPC_REBEL_SFW6R-1ST">
<description>FCI FPC connector SFW6R-1STE1LF

according to Drawing JSA 96336 / revision D, Nov 1, 2009

used in Rebelsim FPC</description>
</package>
<package name="WEEE_BIN_TOP">
<description>WEEE bin according to Article 11(2) of the WEEE directive</description>
</package>
<package name="WEEE_BIN">
</package>
</packages>
</library>
<library name="rc-sysmocom">
<packages>
<package name="_0603">
<description>&lt;b&gt;0603&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="oshw">
<description>&lt;p&gt;&lt;strong&gt;Open Source Hardware PCB Logos&lt;/strong&gt;
&lt;p&gt;A simple polygon based version of the OSHWA logos for use on Eagle PCB's
&lt;p&gt;For use please refer to the OSHWA definition at &lt;a href="http://www.oshwa.org/definition/"&gt;http://www.oshwa.org/definition/&lt;/a&gt;
&lt;p&gt;Based on the NBitWonder version (&lt;a href="http://nbitwonder.com"&gt;http://nbitwonder.com&lt;/a&gt;)
&lt;p&gt;&lt;strong&gt;Andrew Cooper&lt;/strong&gt;&lt;br&gt;28Nov2016&lt;br&gt;&lt;a href="http://www.darkerview.com"&gt;www.DarkerView.com&lt;/a&gt;</description>
<packages>
<package name="OSHW_8MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="iso7816-card" package="ISO7816_CARD" value=""/>
<element name="X2" library="laforge" package="FPC_REBEL_SFW6R-1ST" value="FCI_FPC_REBEL_SFW6R-1">
<attribute name="OC_DIGIKEY" value="609-1889-1-ND"/>
</element>
<element name="C1" library="rc-sysmocom" package="_0603" value=""/>
<element name="U$1" library="laforge" package="WEEE_BIN_TOP" value=""/>
<element name="U$2" library="laforge" package="WEEE_BIN" value=""/>
<element name="U$3" library="oshw" package="OSHW_8MM" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="X2" pad="1"/>
<contactref element="X1" pad="C1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="RST">
<contactref element="X2" pad="2"/>
<contactref element="X1" pad="C2"/>
</signal>
<signal name="CLK">
<contactref element="X2" pad="3"/>
<contactref element="X1" pad="C3"/>
</signal>
<signal name="GND">
<contactref element="X1" pad="C5"/>
<contactref element="X2" pad="6"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="VPP">
<contactref element="X1" pad="C6"/>
<contactref element="X2" pad="5"/>
</signal>
<signal name="IO">
<contactref element="X1" pad="C7"/>
<contactref element="X2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
