INFO: Using PC/SC reader interface
Reading ...
Autodetected card type: Fairwaves-SIM
ICCID: 8988219000000117833
IMSI: 001010000000111
GID1: ffffffffffffffff
GID2: ffffffffffffffff
SMSP: ffffffffffffffffffffffffffffe1ffffffffffffffffffffffff0581005155f5ffffffffffff000000
SMSC: 0015555
SPN: Fairwaves
Show in HPLMN: False
Hide in OPLMN: False
PLMNsel: ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
PLMNwAcT:
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused

OPLMNwAcT:
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused

HPLMNAcT:
	00f110ffff # MCC: 001 MNC: 01 AcT: E-UTRAN NB-S1, E-UTRAN WB-S1, EC-GSM-IoT, GSM, GSM COMPACT, NG-RAN, UTRAN, cdma2000 1xRTT, cdma2000 HRPD
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused

ACC: 0008
MSISDN: Not available
Administrative data: 00000002
	MS operation mode: normal
	Ciphering Indicator: disabled
SIM Service Table: ff3cc3ff030fff0f000fff03f0c0
	Service 1 - CHV1 disable function
	Service 2 - Abbreviated Dialling Numbers (ADN)
	Service 3 - Fixed Dialling Numbers (FDN)
	Service 4 - Short Message Storage (SMS)
	Service 5 - Advice of Charge (AoC)
	Service 6 - Capability Configuration Parameters (CCP)
	Service 7 - PLMN selector
	Service 8 - RFU
	Service 11 - Extension2
	Service 12 - SMS Parameters
	Service 13 - Last Number Dialled (LND)
	Service 14 - Cell Broadcast Message Identifier
	Service 17 - Service Provider Name
	Service 18 - Service Dialling Numbers (SDN)
	Service 23 - enhanced Multi-Level Precedence and Pre-emption Service
	Service 24 - Automatic Answer for eMLPP
	Service 25 - Data download via SMS-CB
	Service 26 - Data download via SMS-PP
	Service 27 - Menu selection
	Service 28 - Call control
	Service 29 - Proactive SIM
	Service 30 - Cell Broadcast Message Identifier Ranges
	Service 31 - Barred Dialling Numbers (BDN)
	Service 32 - Extension4
	Service 33 - De-personalization Control Keys
	Service 34 - Co-operative Network List
	Service 41 - USSD string data object supported in Call Control
	Service 42 - RUN AT COMMAND command
	Service 43 - User controlled PLMN Selector with Access Technology
	Service 44 - Operator controlled PLMN Selector with Access Technology
	Service 49 - MExE
	Service 50 - Reserved and shall be ignored
	Service 51 - PLMN Network Name
	Service 52 - Operator PLMN List
	Service 53 - Mailbox Dialling Numbers
	Service 54 - Message Waiting Indication Status
	Service 55 - Call Forwarding Indication Status
	Service 56 - Service Provider Display Information
	Service 57 - Multimedia Messaging Service (MMS)
	Service 58 - Extension 8
	Service 59 - MMS User Connectivity Parameters

FPLMN:
	ffffff # unused
	ffffff # unused
	ffffff # unused
	ffffff # unused
	ffffff # unused
	ffffff # unused
	ffffff # unused
	ffffff # unused
	ffffff # unused
	ffffff # unused

USIM Service Table: 01ea1ffc21360480010000
	Service 1 - Local Phone Book
	Service 10 - Short Message Storage (SMS)
	Service 12 - Short Message Service Parameters (SMSP)
	Service 14 - Capability Configuration Parameters 2 (CCP2)
	Service 15 - Cell Broadcast Message Identifier
	Service 16 - Cell Broadcast Message Identifier Ranges
	Service 17 - Group Identifier Level 1
	Service 18 - Group Identifier Level 2
	Service 19 - Service Provider Name
	Service 20 - User controlled PLMN selector with Access Technology
	Service 21 - MSISDN
	Service 27 - GSM Access
	Service 28 - Data download via SMS-PP
	Service 29 - Data download via SMS-CB
	Service 30 - Call Control by USIM
	Service 31 - MO-SMS Control by USIM
	Service 32 - RUN AT COMMAND command
	Service 33 - shall be set to 1
	Service 38 - GSM security context
	Service 42 - Operator controlled PLMN selector with Access Technology
	Service 43 - HPLMN selector with Access Technology
	Service 45 - PLMN Network Name
	Service 46 - Operator PLMN List
	Service 51 - Service Provider Display Information
	Service 64 - VGCS security
	Service 65 - VBS security

Done !

