INFO: Using PC/SC reader interface
Reading ...
Autodetected card type: sysmoUSIM-SJS1
ICCID: 8988211320300000028
IMSI: 001010000000102
GID1: ffffffffffffffffffff
GID2: ffffffffffffffffffff
SMSP: ffffffffffffffffffffffffffffffffffffffffffffffffe1ffffffffffffffffffffffff0581005155f5ffffffffffff000000
SMSC: 0015555
SPN: Magic
Show in HPLMN: True
Hide in OPLMN: True
PLMNsel: 00f110ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
PLMNwAcT:
	00f110ffff # MCC: 001 MNC: 01 AcT: E-UTRAN NB-S1, E-UTRAN WB-S1, EC-GSM-IoT, GSM, GSM COMPACT, NG-RAN, UTRAN, cdma2000 1xRTT, cdma2000 HRPD
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused

OPLMNwAcT:
	00f110ffff # MCC: 001 MNC: 01 AcT: E-UTRAN NB-S1, E-UTRAN WB-S1, EC-GSM-IoT, GSM, GSM COMPACT, NG-RAN, UTRAN, cdma2000 1xRTT, cdma2000 HRPD
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused

HPLMNAcT:
	00f110ffff # MCC: 001 MNC: 01 AcT: E-UTRAN NB-S1, E-UTRAN WB-S1, EC-GSM-IoT, GSM, GSM COMPACT, NG-RAN, UTRAN, cdma2000 1xRTT, cdma2000 HRPD
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused
	ffffff0000 # unused

ACC: 0008
MSISDN (NPI=1 ToN=1): +77776336143
Administrative data: 00000002
	MS operation mode: normal
	Ciphering Indicator: disabled
SIM Service Table: ff3fffff3f003f1ff00c00c0f00000
	Service 1 - CHV1 disable function
	Service 2 - Abbreviated Dialling Numbers (ADN)
	Service 3 - Fixed Dialling Numbers (FDN)
	Service 4 - Short Message Storage (SMS)
	Service 5 - Advice of Charge (AoC)
	Service 6 - Capability Configuration Parameters (CCP)
	Service 7 - PLMN selector
	Service 8 - RFU
	Service 9 - MSISDN
	Service 10 - Extension1
	Service 11 - Extension2
	Service 12 - SMS Parameters
	Service 13 - Last Number Dialled (LND)
	Service 14 - Cell Broadcast Message Identifier
	Service 17 - Service Provider Name
	Service 18 - Service Dialling Numbers (SDN)
	Service 19 - Extension3
	Service 20 - RFU
	Service 21 - VGCS Group Identifier List (EFVGCS and EFVGCSS)
	Service 22 - VBS Group Identifier List (EFVBS and EFVBSS)
	Service 23 - enhanced Multi-Level Precedence and Pre-emption Service
	Service 24 - Automatic Answer for eMLPP
	Service 25 - Data download via SMS-CB
	Service 26 - Data download via SMS-PP
	Service 27 - Menu selection
	Service 28 - Call control
	Service 29 - Proactive SIM
	Service 30 - Cell Broadcast Message Identifier Ranges
	Service 31 - Barred Dialling Numbers (BDN)
	Service 32 - Extension4
	Service 33 - De-personalization Control Keys
	Service 34 - Co-operative Network List
	Service 35 - Short Message Status Reports
	Service 36 - Network's indication of alerting in the MS
	Service 37 - Mobile Originated Short Message control by SIM
	Service 38 - GPRS
	Service 49 - MExE
	Service 50 - Reserved and shall be ignored
	Service 51 - PLMN Network Name
	Service 52 - Operator PLMN List
	Service 53 - Mailbox Dialling Numbers
	Service 54 - Message Waiting Indication Status
	Service 57 - Multimedia Messaging Service (MMS)
	Service 58 - Extension 8
	Service 59 - MMS User Connectivity Parameters

FPLMN:
	62f201 # MCC: 262 MNC: 10
	62f202 # MCC: 262 MNC: 20
	62f203 # MCC: 262 MNC: 30
	62f207 # MCC: 262 MNC: 70

USIM Service Table: 9e6b1dfc67f6580000
	Service 2 - Fixed Dialling Numbers (FDN)
	Service 3 - Extension 2
	Service 4 - Service Dialling Numbers (SDN)
	Service 5 - Extension3
	Service 8 - Outgoing Call Information (OCI and OCT)
	Service 9 - Incoming Call Information (ICI and ICT)
	Service 10 - Short Message Storage (SMS)
	Service 12 - Short Message Service Parameters (SMSP)
	Service 14 - Capability Configuration Parameters 2 (CCP2)
	Service 15 - Cell Broadcast Message Identifier
	Service 17 - Group Identifier Level 1
	Service 19 - Service Provider Name
	Service 20 - User controlled PLMN selector with Access Technology
	Service 21 - MSISDN
	Service 27 - GSM Access
	Service 28 - Data download via SMS-PP
	Service 29 - Data download via SMS-CB
	Service 30 - Call Control by USIM
	Service 31 - MO-SMS Control by USIM
	Service 32 - RUN AT COMMAND command
	Service 33 - shall be set to 1
	Service 34 - Enabled Services Table
	Service 35 - APN Control List (ACL)
	Service 38 - GSM security context
	Service 39 - CPBCCH Information
	Service 42 - Operator controlled PLMN selector with Access Technology
	Service 43 - HPLMN selector with Access Technology
	Service 45 - PLMN Network Name
	Service 46 - Operator PLMN List
	Service 47 - Mailbox Dialling Numbers
	Service 48 - Message Waiting Indication Status
	Service 52 - Multimedia Messaging Service (MMS)
	Service 53 - Extension 8
	Service 55 - MMS User Connectivity Parameters

Done !

